R11-13G-S4810-1#show running-config

Current Configuration ...

Version 9.2(0.0)

Last configuration change at Thu Mar 12 02:41:08 2015 by crowbar

Startup-config last updated at Mon Mar 9 07:07:36 2015 by crowbar

boot system stack-unit 0 primary system: A:

boot system stack-unit 0 secondary system: B:

boot system stack-unit 0 default system: A:

redundancy auto-synchronize full

hardware watchdog

logging console informational

hostname R11-13G-S4810-1

username userxx password xxxxxxx privilege 15

protocol spanning-tree rstp

no disable

bridge-priority 8192

vlt domain 11

peer-link port-channel 11

back-up destination 10.9.244.53

primary-priority 4096

unit-id 0

stack-unit 0 provision S4810

interface TenGigabitEthernet 0/0

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/1

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/2

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/3

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/4

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/5

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/6

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/7

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/8

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/9

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/10

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/11

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/12

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/13

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/14

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/15

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/16

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/17

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/18

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/19

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/20

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/21

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/22

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/23

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/24

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/25

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/26

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/27

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/28

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/29

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/30

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/31

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/32

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/33

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/34

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/35

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/36

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/37

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/38

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/39

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/40

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/41

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/42

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/43

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/44

description VLAN120-SAHPXE

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/45

no ip address

mtu 12000

portmode hybrid

switchport

flowcontrol rx on tx off

spanning-tree rstp edge-port

no shutdown

interface TenGigabitEthernet 0/46

no ip address

mtu 12000

no shutdown

interface TenGigabitEthernet 0/47

no ip address

mtu 12000

no shutdown

interface fortyGigE 0/48

no ip address

mtu 12000

flowcontrol rx on tx on

no shutdown

interface fortyGigE 0/52

no ip address

mtu 12000

flowcontrol rx on tx on

no shutdown

interface fortyGigE 0/56

no ip address

no shutdown

interface fortyGigE 0/60

no ip address

no shutdown

interface ManagementEthernet 0/0

ip address 10.9.244.52/23

no shutdown

interface ManagementEthernet 1/0

no shutdown

interface ManagementEthernet 2/0

no shutdown

interface ManagementEthernet 3/0

no shutdown

interface ManagementEthernet 4/0

no shutdown

interface ManagementEthernet 5/0

no shutdown

interface ManagementEthernet 6/0

no shutdown

interface ManagementEthernet 7/0

no shutdown

interface ManagementEthernet 8/0

no shutdown

interface ManagementEthernet 9/0

no shutdown

interface ManagementEthernet 10/0

no shutdown

interface ManagementEthernet 11/0

no shutdown

interface Port-channel 11

description R11-13G-VLT

no ip address

mtu 12000

channel-member fortyGigE 0/48,52

no shutdown

interface Port-channel 55

no ip address

switchport

channel-member TenGigabitEthernet 0/46

vlt-peer-lag port-channel 55

no shutdown

interface Port-channel 111

description Uplink\_NGN-Core

no ip address

switchport

channel-member TenGigabitEthernet 0/47

vlt-peer-lag port-channel 111

no shutdown

interface Vlan 1

untagged TenGigabitEthernet 0/0-6,10-11,22-34,37-45

untagged Port-channel 11

interface Vlan 110

description iDRACs\_13G

no ip address

tagged TenGigabitEthernet 0/36,44-45

tagged Port-channel 55

no shutdown

interface Vlan 120

description Provisioner

ip address 192.168.120.2/24

tagged TenGigabitEthernet 0/0,36,44-45

tagged Port-channel 55

vrrp-group 120

no preempt

priority 120

virtual-address 192.168.120.1

no shutdown

interface Vlan 140

description Private\_API

ip address 192.168.140.1/24

tagged TenGigabitEthernet 0/1-6,36,44-45

no shutdown

interface Vlan 157

description NGN\_Public\_API

no ip address

tagged Port-channel 55,111

untagged TenGigabitEthernet 0/12,36

no shutdown

interface Vlan 158

description SAHs\_iDRAC

no ip address

tagged Port-channel 55,111

no shutdown

interface Vlan 170

description Storage

ip address 192.168.170.1/24

tagged TenGigabitEthernet 0/0-3,36

tagged Port-channel 55

untagged TenGigabitEthernet 0/7-9,16-18,35

no shutdown

interface Vlan 180

description Ceph\_Cluster

ip address 192.168.180.1/24

tagged TenGigabitEthernet 0/36

untagged TenGigabitEthernet 0/19-21

no shutdown

interface Vlan 190

description Nova\_Net\_Public

ip address 192.168.190.254/24

tagged TenGigabitEthernet 0/36

untagged TenGigabitEthernet 0/13-15

no shutdown

interface Vlan 201

description Nova\_Net\_Private

ip address 192.168.201.254/24

tagged TenGigabitEthernet 0/1-6,16-18,36

no shutdown

interface Vlan 202

description Nova\_Net\_Private

no ip address

tagged TenGigabitEthernet 0/1-6,36

no shutdown

interface Vlan 203

description Nova\_Net\_Private

no ip address

tagged TenGigabitEthernet 0/1-6,36

no shutdown

interface Vlan 204

description Nova\_Net\_Private

no ip address

tagged TenGigabitEthernet 0/1-6,36

no shutdown

interface Vlan 205

description Nova\_Net\_Private

no ip address

tagged TenGigabitEthernet 0/1-6,36

no shutdown

interface Vlan 206

description Nova\_Net\_Private

no ip address

tagged TenGigabitEthernet 0/1-6,36

no shutdown

interface Vlan 207

description Nova\_Net\_Private

no ip address

tagged TenGigabitEthernet 0/1-6,36

no shutdown

interface Vlan 208

description Nova\_Net\_Private

no ip address

tagged TenGigabitEthernet 0/1-6,36

no shutdown

interface Vlan 209

description Nova\_Net\_Private

no ip address

tagged TenGigabitEthernet 0/1-6,36

no shutdown

interface Vlan 210

description Nova\_Net\_Private

no ip address

tagged TenGigabitEthernet 0/1-6,36

no shutdown

interface Vlan 211

description Nova\_Net\_Private

no ip address

tagged TenGigabitEthernet 0/1-6,36

no shutdown

interface Vlan 212

description Nova\_Net\_Private

no ip address

tagged TenGigabitEthernet 0/1-6,36

no shutdown

interface Vlan 213

description Nova\_Net\_Private

no ip address

tagged TenGigabitEthernet 0/1-6,36

no shutdown

interface Vlan 214

description Nova\_Net\_Private

no ip address

tagged TenGigabitEthernet 0/1-6,36

no shutdown

interface Vlan 215

description Nova\_Net\_Private

no ip address

tagged TenGigabitEthernet 0/1-6,36

no shutdown

interface Vlan 216

description Nova\_Net\_Private

no ip address

tagged TenGigabitEthernet 0/1-6,36

no shutdown

interface Vlan 217

description Nova\_Net\_Private

no ip address

tagged TenGigabitEthernet 0/1-6,36

no shutdown

interface Vlan 218

description Nova\_Net\_Private

no ip address

tagged TenGigabitEthernet 0/1-6,36

no shutdown

interface Vlan 219

description Nova\_Net\_Private

no ip address

tagged TenGigabitEthernet 0/1-6,36

no shutdown

interface Vlan 220

description Nova\_Net\_Private

no ip address

tagged TenGigabitEthernet 0/1-6,36

no shutdown

management route 0.0.0.0/0 10.9.244.1

no ip telnet server enable

ip ssh server enable

protocol lldp

advertise dot1-tlv port-protocol-vlan-id

advertise dot3-tlv max-frame-size

advertise management-tlv system-description system-name

advertise med

line console 0

line vty 0

line vty 1

line vty 2

line vty 3

line vty 4

line vty 5

line vty 6

line vty 7

line vty 8

line vty 9

reload-type normal-reload

end

R11-13G-S4810-1#