Some Important Points for s6000 Configuration:

• Splitting a 40G port into 4x10G port is supported only on a standalone unit.

• Split ports cannot be used as stack-link to stack an S6000.

• Split ports cannot be a part of any stacked system.

• Few of the Ports in S6000 are fixed 40G Ports and hence splitting is not allowed. Fixed Port nos are (4,12,20,28,100,108,116,124)

**Command to split interface: stack-unit 0 port 48 portmade quad**

• Reload is mandatory when QSFP ports are converted into 4\*10G SFP+ ports using portmode quad cli and the same for converting back quad ports to QSFP Port